


Use the check-off method to wire the provided components according to this schematic.









**Relay  
(M1)**